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$250/20(SAP) TECHNICAL DATASHEET

TECHNICAL SPECIFICATIONS- CANOPY DESIGN (SAP)

Wodel 5250/20 Pump Model CRP150DP240T ENSSK
um Flow (m3/hi) 450 ‘Wet End Materials GGG4 Ductle Iron
‘Maximum Head (m) 50 impeller GGG4 Ductle Iron
WMax solids Handling (mm) 76 ‘Wear Ring Gastron
um Efficiency (%) &0 Shaft 17-4PH Stainless Steel
um Lt (m) 85 Bearing Housing Cast ron
um Speed (rpm) 1800 Mechanical Seal Cycloseal o/w run-dry
um Power (kw) 2 Priming pump. 50cim diaphragm vacuum
Best Efficiency Point 250m3/hr ot 20m | SAE Housing 4
Power at BEP (k) 185 Drive Size 0inch
Fuel Consumption (Iph) 3 Front Bearing Roller
Fuel Tank Size (itres) 240 Drive Bearing(s] Single
Sound Rating (dbA)@7m [
Dimensions (LxWxH) m 23m10mx 1.7m | Engine Tsuzu
Weight (Dry) (kg) 1800 Make aLEL
Size 221t
Power 23kw

Dimensions are for guidance only. Exact dimensions can be acquired from the factory. Other
configurations such as canopy units may well have different dimensions.

Always check with DXB Pump & Power Limited





